Tips for updating and working with Alpha-Bio Tec. libraries

1. Before installing the new libraries, please delete all old libraries
2. There are 4 main libraries which correspond to the connections and the scan body used.
   * + Alpha-Bio\_Tec\_CS
     + Alpha-Bio\_Tec\_IH\_and\_CHC\_7mm\_Scan\_Body
     + Alpha-Bio\_Tec\_IH\_and\_CHC\_10mm\_Scan\_Body
     + Alpha-Bio\_Tec\_TCT (Multi-unit)

There are 2 scan bodies:

* 1. TCT-N-R rotational (for bridges) – 7mm
  2. TCT-N anti-rotational (for single crowns on angled abutments) – 7mm, 10mm   
       
     Note: although it is recommended to use the TCT-N-R for bridges, the libraries also support scans with the AR scan body

1. Model creator library
   * + Alpha-Bio\_Tec\_CS
     + Alpha-Bio\_Tec\_IH
     + Alpha-Bio\_Tec\_CHC